# Lab 06 Perform straight drilling to calculate Material removal rate and machining time.

# Required:

1. Plot a relationship between RPMs and Feed Rate.
2. Plot a relationship between RPMs and Material Removal Rate.
3. Plot a relationship between RPMs and Machining time.
4. Plot a relationship between RPMs and Actual Machining time.
5. Plot a relationship between machining time and actual time.

# MATLAB CODE:

% Student: (Barira Qasim - F2022031016)

% Given Data

L = [23.3, 25.15, 25.15, 25.15, 25.15, 25.15]; % Depth of hole in mm

D = [2, 16, 16, 16, 16, 16]; % Diameter of drill bit in mm

RPMs = [420, 660, 660, 660, 660, 660]; % RPMs

feed\_rate = [43, 43, 43, 43, 43, 43]; % Feed Rate in mm/min

MRR = [135, 8646, 8646, 8646, 8646, 8646]; % Material Removal Rate in mm^3/min

machining\_time = [0.561162791, 0.604186047, 0.604186047, 0.604186047, 0.604186047, 0.604186047]; % Machining Time in min

actual\_machining\_time = [1.37, 0.67, 0.68, 0.61, 0.72, 0.77]; % Actual Machining Time in min

% Plotting Relationships

% 1. Plot: RPMs vs Feed Rate

figure;

plot(RPMs, feed\_rate, '-x', 'LineWidth', 2);

xlabel('RPM (rev/min)');

ylabel('Feed Rate (mm/min)');

title('Lab 06: RPMs vs Feed Rate (Barira Qasim - F2022031016)');

legend('Feed Rate vs RPMs');

grid on;

% 2. Plot: RPMs vs Material Removal Rate

figure;

plot(RPMs, MRR, '-x', 'LineWidth', 2);

xlabel('RPM (rev/min)');

ylabel('Material Removal Rate (mm^3/min)');

title('Lab 06: RPMs vs Material Removal Rate (Barira Qasim - F2022031016)');

legend('Material Removal Rate vs RPMs');

grid on;

% 3. Plot: RPMs vs Machining Time

figure;

plot(RPMs, machining\_time, '-x', 'LineWidth', 2);

xlabel('RPM (rev/min)');

ylabel('Machining Time (min)');

title('Lab 06: RPMs vs Machining Time (Barira Qasim - F2022031016)');

legend('Machining Time vs RPMs');

grid on;

% 4. Plot: RPMs vs Actual Machining Time

figure;

plot(RPMs, actual\_machining\_time, '-x', 'LineWidth', 2);

xlabel('RPM (rev/min)');

ylabel('Actual Machining Time (min)');

title('Lab 06: RPMs vs Actual Machining Time (Barira Qasim - F2022031016)');

legend('Actual Machining Time vs RPMs');

grid on;

% 5. Plot: Machining Time vs Actual Machining Time

figure;

plot(machining\_time, actual\_machining\_time,'-x', 'LineWidth', 2);


xlabel('Machining Time (min)');





ylabel('Actual Machining Time (min)');

title('Lab 06: Machining Time vs Actual Machining Time (Barira Qasim - F2022031016)');

legend('Actual Time vs Machining Time');

grid on;

Graphs



# Comments:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_